B205 PRODUCT INFORMATION B205

FLEETWASH 600

TRAFFIC FILM REMOVER CONCENTRATE

PRODUCT DESCRIPTION

B205 is a combination of surface active agents, sequestrants, and alkaline builders designed for use in cleaning vehicles, through hot or cold water pressure washer systems. The product is caustic soda free and will not affect paintwork. The water softeners in the formulation boost the cleaning properties in hard water areas and also reduce scale build up within the equipment. B205 works under normal conditions without agitation

PRODUCT DILUTION

B205 can be diluted up to 600-1 with hot or cold water depending on the severity of the cleaning needed. It can be used through pressure washer systems or manually if preferred. The diluted product is applied to the surface liberally and washed away with water. Leathering is not normally required.

PRODUCT APPLICATION

B205 is used for cleaning all traffic grime from all vehicles. It will clean engines and chassis when used through pressure washer systems. Also used as a powerful hard surface cleaner and forecourt cleaner.

